A fume hood used for Beta and Gamma radiation shall be referred to as a radioisotope hood. The Kewaunee Supreme Air Venturi radioisotope hood has the general characteristics of a bench-top fume hood except the work surface and interior lining shall be type 304 stainless steel with coved seamless welded seams for easy cleaning and decontamination. The hood design is identical to other hood types in nearly all other respects.

Compliance : ASHRAE 110 , EN-14175-3

Sizes : 4 Feet, 5 Feet, 6 Feet, 8 Feet

Sash : Vertical

Liner : Type 304L Stainless Steel

Bypass : Open, Restricted